**Emergency Eyewash Station**

**Weekly Inspection Checklist**

# How to Inspect & Test:

* Is the area around the station clear of obstructions?
* Is the eyewash clean and free of dirt/debris?
* Flush eyewash for 30 seconds weekly
* Do the covers/caps open without assistance?
* Is the plumbing free from leakage?
* Are the jets working properly (both spigots are delivering evenly, and with sufficient but not too great of a flow)?
* Is the water clean and clear?

# How to Obtain Assistance:

## Questions, maintenance, training

**EHS:** 302-831-8475 | [dehsafety@udel.edu](mailto:dehsafety@udel.edu)

## Maintenance

requests may also be called in directly

**Facilities Services**: 302-831-1141

## Emergencies:

Hold eyes open and flush for at least 15 minutes. CALL 911 and seek medical assistance

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| ***Date*** | ***Initials*** | ***Comment*** |  | ***Date*** | ***Initials*** | ***Comment*** |
|  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |